So, this is closer view of HOTO box.

Here it has 5 physical buttons to turn on and off sensors and corresponding LEDs to show the status.

And there is an implemented camera at the front of the box.

also, each side has two electricity outlets for electric supply.

Then, 4 USB ports in the back for our sensor modules.

As mentioned in the presentation, it has three phases which are ‘SENSOR OFF’, ‘SENSOR ON’ and ‘AUTO MODE’.

We are going to demonstrate phase by phase. Let us start by SENSOR OFF mode.